<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<packages>
<package name="SOP50P505X110-10N-RWD">
<description>10-SOP, 0.50 mm pitch, 5.05 mm span, 3.10 X 3.10 X 1.10 mm body
10-pin SOP package with 0.50 mm pitch, 5.05 mm span with body size 3.10 X 3.10 X 1.10 mm</description>
</package>
</packages>
<symbols>
<symbol name="ADS1115IDGSR">
<pin name="ADDR" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="VDD" direction="pwr"/>
<pin name="ALERT/RDY" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RWD-ADS1115IDGSR" prefix="U">
<description> &lt;a href="https://pricing.snapeda.com/parts/ADS1115IDGSR/Texas%20Instruments/view-part?ref=eda"&gt;Check availability&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1115IDGSR"/>
</gates>
<devices>
<device name="ADS1115IDGSR" package="SOP50P505X110-10N-RWD">
<connects>
<connect gate="G$1" pin="ADDR" pad="1"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="ALERT/RDY" pad="6"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCL" pad="8"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
